{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"not_rendered":{"charts":0,"images":25,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":35,"n_cols":35,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[{"$nulls":5},"Mosfet "]
[{"$nulls":5},"(N-Kanal Isolierschicht-Feldeffekttransistor)"]
[]
[{"$nulls":5},"Widerstand allgemein",{"$nulls":16},"Motor EL"]
[]
[{"$nulls":15},"-",{"$nulls":18},"+"]
[{"$nulls":5},"Kondensator allgemein"]
[]
[{"$nulls":19},"Strang 1 "]
[]
[{"$nulls":5},"Akku"]
[{"$nulls":23},"20A"]
[]
[]
[{"$nulls":5},"Schalter normal"]
[{"$nulls":27},"48V NC"]
[]
[]
[{"$nulls":5},"Zehnerdiode"]
[{"$nulls":29},"S"]
[]
[{"$nulls":5},"Diode allgemein"]
[]
[{"$nulls":5},"Schottkydiode",{"$nulls":20},"G"]
[]
[{"$nulls":5},"Sicherung"]
[]
[{"$nulls":5},"Verbindung"]
[{"$nulls":28},"D"]
[]
[{"$nulls":5},"?",{"$nulls":19},"G"]
[{"$nulls":16},"+",{"$nulls":11},"S"]
[{"$nulls":18},"Laden"]
[{"$nulls":18},"45 - 48V"]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}